EXPRESSION OF INTEREST (EOI)

**EOI Reference #: ASMC-WRTI-EOI-2023-009**

**Title: SE811 – In-Dock Mooring System Rigging**

**Project: West White Rose CGS Tow-out & Installation**

**Issue Date:** August 10, 2023

**Closing Date:** August 24, 2023

**GENERAL**

Aker Solutions Marine Contractors Limited (ASMC) hereby invites interested parties to submit an Expression of Interest (EOI) related to the future Requests for Tender for the following Scope of Work in connection with ASMC Concrete Gravity Structure (CGS) Tow-out and Installation Scope of Work for the Cenovus West White Rose Project in Newfoundland and Labrador, Canada.

**BENEFITS COMMITMENTS**

ASMC is committed to providing full and fair opportunities to commercially competitive Canadian companies with first consideration given to those from Newfoundland and Labrador. At the Pre-Qualification and ITT stages, companies will be required to complete Canada/Newfoundland & Labrador Benefits questionnaires to acknowledge their willingness to comply with the White Rose Canada-Newfoundland and Labrador Benefits Plan.

**EQUAL OPPORTUNITY**

ASMC is an equal opportunity employer and supports diversity in the workplace. Successful suppliers and subcontractors to ASMC will be required to undertake a commitment to support diversity in execution of work on the West White Rose Project.

**SCOPE OF SERVICES**

ASMC requires the provision of an in-door mooring system to be used while the CGS is afloat in the graving dock, prior to tow and installation of the CGS. The equipment required will include the following:

* 24-off Ø48mm 6x36 EEIP IWRC wire ropes of various length ranging from 20m to 98m; total length ~1000m
  + Requires “3.2 certification”
* 12-off Ø54mm stud less chain segments of various length ranging from 24m to 72m; total length ~430m,
* 26-off 55Te bolt type anchor shackles, Crosby G-2130 or similar
* 23-off 17Te bolt type anchor shackles, Crosby G-2130 or similar
* 12-off Ø25mm 6x36 EEIP IWRC wire ropes, 25m length; total length 300m
* 2-off chafe protection sleeves to suit Ø48mm wire rope, 5m length each

OPTION: ASMC may elect to increase the Ø48mm wire rope to Ø51mm – TBD.

Used equipment may be considered, provided it is recently inspected and certified by a qualified third party.

Note: All equipment shall be certified in accordance with industry standards. Wire rope slings may require load testing, and applicable documentation demonstrating proof of testing will be required to be submitted for review.

**SCHEDULE AND DELIVERY**

**Required On Site date (Tentative): May 2024**

Delivery Location: CGS Construction Site at Argentia, NL

**SUBMISSION REQUIREMENTS**

As part of the submission requirements, suppliers are requested to provide Aker Solutions Marine Contractors Limited with the following answers and/or information:

1. Please provide a brief outline of the following company information:
   1. Copy of Certificate of Incorporation.
   2. Company Name and Address.
   3. Single Point of Contact, c/w contact details.
2. A list of previous work experience related directly to the scope of services including supply, testing and certification of rigging suitable for use in a marine environment as well as relevant experience coordinating third-party certification e.g., DNV, CSA, etc. This list should include but not be limited to the client’s name, project date, location, specific industry sector and proposed manufacturer.
3. Overview of your company’s equipment and tools maintenance and calibration/recertification program with specific reference to the database being used to manage this.
4. Please provide a brief description and overview of the execution plan, facility(ies) being proposed to execute the work, manufacturing locations and sub-supplier(s). Also, please provide details related to work that will be subcontracted (if any) and outline the expected scopes and subcontractor options (names and locations).

**RESPONSE REQUIREMENTS**

Suppliers are to respond to the following e-mail address: [ASMC.WRTI\_Procurement@akersolutions.com](mailto:ASMC.WRTI_Procurement@akersolutions.com)

on or before the closing date noted above.

The subject line of the email must contain the following:

**EOI REFERNCE NUMBER – TITLE – Supplier Company Name**

Suppliers that have not been pre-qualified will be required to do so before the formal RFQ/Tender/Bid packages.

If you have any questions regarding this announcement, please contact Aker Solutions Single Point of Contact listed below:

Tanya O’Neill

Contracts Manager

Aker Solutions Marine Contractors Limited

[tanya.oneill@akersolutions.com](mailto:tanya.oneill@akersolutions.com)